Selective application of different forming temperatures for individual process stages in a rivet manufacturing process with high nitrogen steel
C.-M. Kuball, B. Uhe, G. Meschut, M. Merklein, in: 2021.
LibreCat: /record/30845

Process design for the forming of semi-tubular self-piercing rivets made of high nitrogen steel
C.-M. Kuball, B. Uhe, G. Meschut, M. Merklein, eds., Process Design for the Forming of Semi-Tubular Self-Piercing Rivets Made of High Nitrogen Steel, 2020.
LibreCat: /record/19976
DOI: 10.1016/j.promfg.2020.08.052

Influence of the process temperature on the forming behaviour and the friction during bulk forming of high nitrogen steel
C.-M. Kuball, R. Jung, B. Uhe, G. Meschut, M. Merklein, eds., Influence of the Process Temperature on the Forming Behaviour and the Friction during Bulk Forming of High Nitrogen Steel, 2020.
LibreCat: /record/19974
DOI: 10.1016/j.jajp.2020.100023

Improvement of a rivet geometry for the self-piercing riveting of high-strength steel and multi-material joints
B. Uhe, C.-M. Kuball, M. Merklein, G. Meschut, Production Engineering 14 (2020) 417–423.
LibreCat: /record/19973
DOI: 10.1007/s11740-020-00973-w

Influence of the process temperature on the tribological behaviour during bulk forming of high nitrogen steel
C.-M. Kuball, R. Jung, B. Uhe, G. Meschut, M. Merklein, in: 2019.
LibreCat: /record/19977