Zinc Anodizing: Structural Diversity of Anodic Zinc Oxide Controlled by the Type of Electrolyte
K. Engelkemeier, A. Sun, D. Voswinkel, O. Grydin, M. Schaper, W. Bremser, ChemElectroChem (2021) 2155–2168.

Thermostable water reservoirs in the interlayer space of a sodium hectorite clay through the intercalation of ;3-aminopropyl(dimethyl)ethoxysilane in toluene
W. Keil, K. Zhao, A. Oswald, W. Bremser, C. Schmidt, H. Hintze-Bruening, Physical Chemistry Chemical Physics 24 (2021) 477–487.

Analytical characterization of polyamide 11 used in the context of selective laser sintering: Physico-chemical correlations
B. Scherer, I.L. Kottenstedde, W. Bremser, F.-M. Matysik, Polymer Testing (2020).

Self-lubricating coatings via PDMS micro-gel dispersions
J. Ressel, O. Seewald, W. Bremser, H.-P. Reicher, O.I. Strube, Progress in Organic Coatings (2020).

Scalable and energy-efficient synthesis of CoxP for overall water splitting in alkaline media by high energy ball milling
H. Xue, H. Zhang, S. Fricke, M. Lüther, Z. Yang, A. Meng, W. Bremser, Z. Li, Sustainable Energy &; Fuels (2019) 1723–1729.