Zinc Anodizing: Structural Diversity of Anodic Zinc Oxide Controlled by the Type of Electrolyte
K. Engelkemeier, A. Sun, D. Voswinkel, O. Grydin, M. Schaper, W. Bremser, ChemElectroChem (2021) 2155–2168.
LibreCat: /record/25272
DOI: 10.1002/celc.202100216

Thermostable water reservoirs in the interlayer space of a sodium hectorite clay through the intercalation of ;3-aminopropyl(dimethyl)ethoxysilane in toluene
W. Keil, K. Zhao, A. Oswald, W. Bremser, C. Schmidt, H. Hintze-Bruening, Physical Chemistry Chemical Physics 24 (2021) 477–487.
LibreCat: /record/35326
DOI: 10.1039/d1cp03321b

Analytical characterization of polyamide 11 used in the context of selective laser sintering: Physico-chemical correlations
B. Scherer, I.L. Kottenstedde, W. Bremser, F.-M. Matysik, Polymer Testing (2020).
LibreCat: /record/25301
DOI: 10.1016/j.polymertesting.2020.106786

Self-lubricating coatings via PDMS micro-gel dispersions
J. Ressel, O. Seewald, W. Bremser, H.-P. Reicher, O.I. Strube, Progress in Organic Coatings (2020).
LibreCat: /record/25302
DOI: 10.1016/j.porgcoat.2020.105705

Scalable and energy-efficient synthesis of CoxP for overall water splitting in alkaline media by high energy ball milling
H. Xue, H. Zhang, S. Fricke, M. Lüther, Z. Yang, A. Meng, W. Bremser, Z. Li, Sustainable Energy &; Fuels (2019) 1723–1729.
LibreCat: /record/25303
DOI: 10.1039/c9se00607a