Schröder, A., and Bernd Henning. .4 - Signal Processing for Single Transducer Distance Measurement Applications to Reduce the Blind Zone. LibreCat University, 2013, doi:10.5162/SENSOR2013/B5.4.

Bause, Fabian, et al. Utilizing Ultrasound Material Parameter Determination for the Characterization of Different Stages of Ageing in Polyamide 6. 2013, pp. 504–09.

Bause, Fabian, et al. Ultrasonic Waveguide Signal Decomposition Using the Synchrosqueezed Wavelet Transform for Modal Group Delay Computation. 2013.

Bause, Fabian, et al. Utilizing Interval-Newton Approach for the Reliable Computation of Roots in Analytical Waveguide Modeling. 2013, pp. 504–09.

Bause, Fabian, et al. “Reliable Computation of Roots in Analytical Waveguide Modeling Using an Interval-Newton Approach and Algorithmic Differentiation.” Transactions on Ultrasonics, Ferroelectrics, and Frequency Control, vol. 60, no. 12, 2013, pp. 2597–606.

Hoof, Christian, et al. “Modellgestützte NIR-Materialfeuchtemessung Mittels Multidetektoranordnung.” Technisches Messen, no. 12, 2013, pp. 435–41.

Hoof, Christian, et al. Untersuchung Zum Trocknungsverhalten Poröser Materialien Durch NIR-Reflexionsmessungen. 2013, pp. 27–38.

Kulshreshtha, Kshitij, et al. A Modified Electrode Topology with Increased Sensitivity of Electrical Impedance to Piezoelectic Material Parameters. 2013.

Schröder, Andreas, and Bernd Henning. “Improved Signal Processing for an Ultrasonic Distance Sensor with Reduced Blind Zone.” Proceedings of the International Conference on Acoustics, DEGA, 2013.

Unverzagt, Carsten, et al. “Modified Electrode Shape for the Improved Determination of Piezoelectric Material Parameters.” Proceedings of the 2013 International Congress on Ultrasonics, edited by Gan Woon Siong et al., Research Publishing, 2013, pp. 758–63.