Multi Reflection of Lamb Wave Emission in an Acoustic Waveguide Sensor
M. Schmitt, S. Olfert, J. Rautenberg, G. Lindner, B. Henning, L. Reindl, Sensors (2013) 2777–2785.

Detection of coatings within liquid-filled tubes and containers by mode conversion of leaky Lamb waves
M. Schmitt, K. Schmidt, S. Olfert, J. Rautenberg, G. Lindner, B. Henning, L.M. Reindl, Journal of Sensors and Sensor Systems (2013) 73–84.

Luftultraschall-Abstandsmessung mit digitaler Signalverarbeitung zur Verkürzung des Mindestabstandes
A. Schröder, B. Henning, tm - Technisches Messen (2013) 196–200.

.4 - Signal Processing for Single Transducer Distance Measurement Applications to Reduce the Blind Zone
A. Schröder, B. Henning, in: LibreCat University, 2013.

Utilizing ultrasound material parameter determination for the characterization of different stages of ageing in Polyamide 6
F. Bause, C. Budde, J. Rautenberg, B. Henning, E. Moritzer, in: 2013, pp. 504–509.

Ultrasonic Waveguide Signal Decomposition Using the Synchrosqueezed Wavelet Transform for Modal Group Delay Computation
F. Bause, B. Huang, A. Kunoth, B. Henning, in: 2013.

Utilizing interval-Newton approach for the reliable computation of roots in analytical waveguide modeling
F. Bause, C. Unverzagt, A. Walther, B. Henning, in: 2013, pp. 504–509.

Reliable Computation of Roots in Analytical Waveguide Modeling Using an Interval-Newton Approach and Algorithmic Differentiation
F. Bause, A. Walther, J. Rautenberg, B. Henning, Transactions on Ultrasonics, Ferroelectrics, and Frequency Control 60 (2013) 2597–2606.

Modellgestützte NIR-Materialfeuchtemessung mittels Multidetektoranordnung
C. Hoof, D. Wetzlar, B. Henning, Technisches Messen (2013) 435–441.

Untersuchung zum Trocknungsverhalten poröser Materialien durch NIR-Reflexionsmessungen
C. Hoof, D. Wetzlar, B. Henning, in: 2013, pp. 27–38.