Haasenritter, J., et al. “Diagnose Im Kontext - Eine Erweiterte Perspektive.” Zeitschrift Für Evidenz, Fortbildung Und Qualität Im Gesundheitswesen (ZEFQ), vol. 107, 2013, pp. 585–91.

Shaker, A., et al. “Evolving Fuzzy Pattern Trees for Binary Classification on Data Streams.” Information Sciences, vol. 220, 2013, pp. 34–45.

Eikel, Benjamin, et al. “Spherical Visibility Sampling.”10.1111/cgf.12150__Computer Graphics Forum, vol. 32, no. 4, 2013, pp. 49–58, doi:10.1111/cgf.12150.

Jähn, Claudius, et al. “Evaluation of Rendering Algorithms Using Position-Dependent Scene Properties.”10.1007/978-3-642-41914-0_12__Advances in Visual Computing, 2013, doi:10.1007/978-3-642-41914-0_12.

Petring, Ralf, et al. “Real-Time 3D Rendering of Heterogeneous Scenes.”10.1007/978-3-642-41914-0_44__Advances in Visual Computing, 2013, doi:10.1007/978-3-642-41914-0_44.

Bause, F., et al. .2 - Design, Modeling and Identification of an Ultrasonic Composite Transducer for Target Impedance Independent Short Pulse Generation. LibreCat University, 2013, doi:10.5162/SENSOR2013/A3.2.

Hoof, C., et al. 3.2 - Infrared Reflectance Measurements of Thin Films with Time Variable Surface Roughness or Texture. LibreCat University, 2013, doi:10.5162/OPTO2013/O3.2.

Rautenberg, Jens, et al. “Messsystem zur Bestimmung akustischer Kenngrößen stark absorbierender, transversal isotroper Kunststoffe.”10.1524/teme.2013.0005__tm - Technisches Messen, 2013, pp. 28–37, doi:10.1524/teme.2013.0005.

Schmitt, Martin, et al. “Multi Reflection of Lamb Wave Emission in an Acoustic Waveguide Sensor.”10.3390/s130302777__Sensors, 2013, pp. 2777–85, doi:10.3390/s130302777.

Schmitt, M., et al. “Detection of Coatings within Liquid-Filled Tubes and Containers by Mode Conversion of Leaky Lamb Waves.”10.5194/jsss-2-73-2013__Journal of Sensors and Sensor Systems, 2013, pp. 73–84, doi:10.5194/jsss-2-73-2013.

Schröder, Andreas, and Bernd Henning. “Luftultraschall-Abstandsmessung mit digitaler Signalverarbeitung zur Verkürzung des Mindestabstandes.”10.1524/teme.2013.0022__tm - Technisches Messen, 2013, pp. 196–200, doi:10.1524/teme.2013.0022.

Schröder, A., and Bernd Henning. .4 - Signal Processing for Single Transducer Distance Measurement Applications to Reduce the Blind Zone. LibreCat University, 2013, doi:10.5162/SENSOR2013/B5.4.

Bause, Fabian, et al. Utilizing Ultrasound Material Parameter Determination for the Characterization of Different Stages of Ageing in Polyamide 6. 2013, pp. 504–09.

Bause, Fabian, et al. Ultrasonic Waveguide Signal Decomposition Using the Synchrosqueezed Wavelet Transform for Modal Group Delay Computation. 2013.

Bause, Fabian, et al. Utilizing Interval-Newton Approach for the Reliable Computation of Roots in Analytical Waveguide Modeling. 2013, pp. 504–09.

Bause, Fabian, et al. “Reliable Computation of Roots in Analytical Waveguide Modeling Using an Interval-Newton Approach and Algorithmic Differentiation.” Transactions on Ultrasonics, Ferroelectrics, and Frequency Control, vol. 60, no. 12, 2013, pp. 2597–606.

Hoof, Christian, et al. “Modellgestützte NIR-Materialfeuchtemessung Mittels Multidetektoranordnung.” Technisches Messen, no. 12, 2013, pp. 435–41.

Hoof, Christian, et al. Untersuchung Zum Trocknungsverhalten Poröser Materialien Durch NIR-Reflexionsmessungen. 2013, pp. 27–38.

Kulshreshtha, Kshitij, et al. A Modified Electrode Topology with Increased Sensitivity of Electrical Impedance to Piezoelectic Material Parameters. 2013.

Schröder, Andreas, and Bernd Henning. “Improved Signal Processing for an Ultrasonic Distance Sensor with Reduced Blind Zone.” Proceedings of the International Conference on Acoustics, DEGA, 2013.