Noé, R., RODLER, H., EBBERG, A., MEISSNER, E., BODLAJ, V., DROGEMULLER, K., &; WITTMANN, J. (1992). FULLY ENGINEERED COHERENT MULTICHANNEL TRANSMITTERS AND RECEIVERS WITH LOW-COST POTENTIAL. ELECTRONICS LETTERS, 28(1), 14–16.https://doi.org/10.1049/el:19920009 
LibreCat: /record/38495
DOI: 10.1049/el:19920009

EBBERG, A., &; Noé, R. (1990). NOVEL HIGH-PRECISION ALIGNMENT TECHNIQUE FOR POLARIZATION MAINTAINING FIBERS USING A FREQUENCY MODULATED TUNABLE LASER. ELECTRONICS LETTERS, 26(24), 2009–2011.https://doi.org/10.1049/el:19901299 
LibreCat: /record/38497
DOI: 10.1049/el:19901299

Noé, R., RODLER, H., GAUKEL, G., EBBERG, A., &; AURACHER, F. (1990). POLARIZATION-INDEPENDENT AND PATTERN-INDEPENDENT OPTICAL FSK HETERODYNE SYSTEM USING DATA-INDUCED POLARIZATION SWITCHING. ELECTRONICS LETTERS, 26(3), 176–177.https://doi.org/10.1049/el:19900119 
LibreCat: /record/38498
DOI: 10.1049/el:19900119

Noé, R., RODLER, H., GAUKEL, G., NOLL, B., &; EBBERG, A. (1990). HIGH-PERFORMANCE, 2-CHANNEL OPTICAL FSK HETERODYNE SYSTEM WITH POLARIZATION DIVERSITY RECEIVER. ELECTRONICS LETTERS, 26(15), 1109–1110.https://doi.org/10.1049/el:19900717 
LibreCat: /record/38501
DOI: 10.1049/el:19900717

Noé, R., GIMLETT, J., VODHANEL, R., &; TSUJI, S. (1989). POLARIZATION-INSENSITIVE, 500 MBIT/S FSK TRANSMISSION OVER 153KM BY PASSIVE POLARIZATION SWITCHING. ELECTRONICS LETTERS, 25(1), 4–5.https://doi.org/10.1049/el:19890003 
LibreCat: /record/38347
DOI: 10.1049/el:19890003

Noé, R., GIMLETT, J., VODHANEL, R., &; TSUJI, S. (1989). POLARIZATION-INSENSITIVE, 500 MBIT/S FSK TRANSMISSION OVER 153KM BY PASSIVE POLARIZATION SWITCHING. ELECTRONICS LETTERS, 25(1), 4–5.https://doi.org/10.1049/el:19890003 
LibreCat: /record/38297
DOI: 10.1049/el:19890003

Noé, R., &; SMITH, D. (1988). INTEGRATED-OPTIC ROTATING WAVEPLATE FREQUENCY SHIFTER. ELECTRONICS LETTERS, 24(21), 1348–1349.https://doi.org/10.1049/el:19880917 
LibreCat: /record/38346
DOI: 10.1049/el:19880917

Noé, R., SESSA, W., WELTER, R., &; KAZOVSKY, L. (1988). NEW FSK PHASE-DIVERSITY RECEIVER IN A 150 MBIT/S COHERENT OPTICAL-TRANSMISSION SYSTEM. ELECTRONICS LETTERS, 24(9), 567–568.https://doi.org/10.1049/el:19880386 
LibreCat: /record/38339
DOI: 10.1049/el:19880386

Noé, R., &; SMITH, D. (1988). INTEGRATED-OPTIC ROTATING WAVEPLATE FREQUENCY SHIFTER. ELECTRONICS LETTERS, 24(21), 1348–1349.https://doi.org/10.1049/el:19880917 
LibreCat: /record/38296
DOI: 10.1049/el:19880917

Noé, R., SESSA, W., WELTER, R., &; KAZOVSKY, L. (1988). NEW FSK PHASE-DIVERSITY RECEIVER IN A 150 MBIT/S COHERENT OPTICAL-TRANSMISSION SYSTEM. ELECTRONICS LETTERS, 24(9), 567–568.https://doi.org/10.1049/el:19880386 
LibreCat: /record/38289
DOI: 10.1049/el:19880386

Noé, R. (1986). ENDLESS POLARIZATION CONTROL EXPERIMENT WITH 3 ELEMENTS OF LIMITED BIREFRINGENCE RANGE. ELECTRONICS LETTERS, 22(25), 1341–1343.https://doi.org/10.1049/el:19860922 
LibreCat: /record/38491
DOI: 10.1049/el:19860922

Noé, R. (1986). ENDLESS POLARIZATION CONTROL IN COHERENT OPTICAL COMMUNICATIONS. ELECTRONICS LETTERS, 22(15), 772–773.https://doi.org/10.1049/el:19860529 
LibreCat: /record/38490
DOI: 10.1049/el:19860529