Wiedemeier, V., Berth, G., Zrenner, A., Larramendi, E. M., Woggon, U., Lischka, K., &; Schikora, D. (2011). In situ characterization of ZnTe epilayer irradiation via time-resolved and power-density-dependent Raman spectroscopy. Semiconductor Science and Technology, 26(10).https://doi.org/10.1088/0268-1242/26/10/105023 

Grynko, Y., Förstner, J., &; Meier, T. (2011). Application of the discontinous Galerkin time domain method to the optics of metallic nanostructures. AAPP | Atti Della Accademia Peloritana Dei Pericolanti, 89(1), Article 1.https://doi.org/10.1478/C1V89S1P041 

Fuchs, C. (2011). Como podemos definir vigilância? MATRIZes, 5(1), 109–133.https://doi.org/10.11606/issn.1982-8160.v5i1p109-136 

Larramendi, E. M., Berth, G., Wiedemeier, V., Hüsch, K.-P., Zrenner, A., Woggon, U.,https://doi.org/10.1088/0268-1242/25/7/075003__Schikora, D. (2010). Intensity enhancement of Te Raman modes by laser damage in ZnTe epilayers. Semiconductor Science and Technology, 25(7).https://doi.org/10.1088/0268-1242/25/7/075003 

Meschut, G. (2005). Mischbauweise sorgt für frischen Wind. Konstruktion, 04, 92–93.

Knop, M., Richter, M., Maßmann, R., Wieser, U., Kunze, U., Reuter, D.,https://doi.org/10.1088/0268-1242/20/8/031__Wieck, A. D. (2005). Preparation of electron waveguide devices on GaAs/AlGaAs using negative-tone resist calixarene. Semiconductor Science and Technology, 814–818.https://doi.org/10.1088/0268-1242/20/8/031 

Kähler, D., Knop, M., Kunze, U., Reuter, D., &; Wieck, A. D. (2004). Dual-gate GaAs/AlGaAs quantum point contact with tuneable subband energy separation. Semiconductor Science and Technology, 140–143.https://doi.org/10.1088/0268-1242/20/2/006 

Apetrii, G., Fischer, S. F., Kunze, U., Reuter, D., &; Wieck, A. D. (2003). Influence of processing parameters on the transport properties of quantum point contacts fabricated with an atomic force microscope. Semiconductor Science and Technology, 735–739.https://doi.org/10.1088/0268-1242/17/7/317 

Hahn, O., Koyro, M., &; Meschut, G. (2002). Lipirea în combinatie cu îmbinarile obtinute prin deformare. Sudura, 2, 10–13.

Reuter, D., Meier, C., Riedesel, C., &; Wieck, A. D. (2002). Local two-dimensional electron gas formation in p-doped GaAs/InyG yAs/AlxG xAs heterostructures by focused Si-implantation doping. Semiconductor Science and Technology, 17(6), 585–589.https://doi.org/10.1088/0268-1242/17/6/315 

Reuter, D., Kähler, D., Kunze, U., &; Wieck, A. D. (2002). Layer-compensated selectively doped AlxG-xAs/GaAs heterostructures as a base material for nanolithography. Semiconductor Science and Technology, 603–607.https://doi.org/10.1088/0268-1242/16/7/314 

Reuter, D., Kähler, D., Kunze, U., &; Wieck, A. D. (2002). Layer-compensated selectively doped AlxG-xAs/GaAs heterostructures as a base material for nanolithography. Semiconductor Science and Technology, 603–607.https://doi.org/10.1088/0268-1242/16/7/314 

Meschut, G. (2001). Hybridfügen – Grundlagen, Technologie, Anwendungen. In DVM-Bericht 668 (Vol. 668, pp. 119–134). Berlin.

Fromme, J., Ganguin, S., Iske, S., Meister, D. M., &; Sander, U. (Eds.). (2000). Medienbildung und Gesellschaft. VS Verlag.

Koyro, M., &; Meschut, G. (1999). Eine quasistationäre Meßmethode zur Ermittlung der Wärmeleitfähigkeit polymerer Zwischenschichten in Abhängigkeit von der Temperatur. In Tagungsband zur Veranstaltung Werkstoffprüfung 1999 (pp. 173–184).

Meier, T., Koch, M., Feldmann, J., Göbel, E. O., Jahnke, F., Schäfer, W., Thomas, P., Koch, S. W., Nickel, H., Luttgen, S., &; Stolz, W. (1994). Coherent Dynamics of Exciton Wavepackets in Semiconductor Heterostructures. Proceedings Der 8. International Winterschool on New Developments in Physics, 9(11S), 1965–1971.https://doi.org/10.1088/0268-1242/9/11S/018