V. Wiedemeier et al., “In situ characterization of ZnTe epilayer irradiation via time-resolved and power-density-dependent Raman spectroscopy,” Semiconductor Science and Technology, vol. 26, no. 10, 2011.

Y. Grynko, J. Förstner, and T. Meier, “Application of the discontinous Galerkin time domain method to the optics of metallic nanostructures,”10.1478/C1V89S1P041__AAPP | Atti della Accademia Peloritana dei Pericolanti, vol. 89, no. 1, Art. no. 1, 2011, doi:10.1478/C1V89S1P041 .

C. Fuchs, “Como podemos definir vigilância?,”https://doi.org/10.11606/issn.1982-8160.v5i1p109-136__MATRIZes, vol. 5, no. 1, pp. 109–133, 2011, doi:https://doi.org/10.11606/issn.1982-8160.v5i1p109-136 .

E. M. Larramendi et al., “Intensity enhancement of Te Raman modes by laser damage in ZnTe epilayers,” Semiconductor Science and Technology, vol. 25, no. 7, 2010.

G. Meschut, “Mischbauweise sorgt für frischen Wind,” Konstruktion, vol. 04, pp. 92–93, 2005.

M. Knop et al., “Preparation of electron waveguide devices on GaAs/AlGaAs using negative-tone resist calixarene,” Semiconductor Science and Technology, pp. 814–818, 2005.

D. Kähler, M. Knop, U. Kunze, D. Reuter, and A. D. Wieck, “Dual-gate GaAs/AlGaAs quantum point contact with tuneable subband energy separation,” Semiconductor Science and Technology, pp. 140–143, 2004.

G. Apetrii, S. F. Fischer, U. Kunze, D. Reuter, and A. D. Wieck, “Influence of processing parameters on the transport properties of quantum point contacts fabricated with an atomic force microscope,” Semiconductor Science and Technology, pp. 735–739, 2003.

O. Hahn, M. Koyro, and G. Meschut, “Lipirea în combinatie cu îmbinarile obtinute prin deformare,” sudura, vol. 2, pp. 10–13, 2002.

D. Reuter, C. Meier, C. Riedesel, and A. D. Wieck, “Local two-dimensional electron gas formation in p-doped GaAs/InyG yAs/AlxG xAs heterostructures by focused Si-implantation doping,” Semiconductor Science and Technology, vol. 17, no. 6, pp. 585–589, 2002.

D. Reuter, D. Kähler, U. Kunze, and A. D. Wieck, “Layer-compensated selectively doped AlxG-xAs/GaAs heterostructures as a base material for nanolithography,” Semiconductor Science and Technology, pp. 603–607, 2002.

D. Reuter, D. Kähler, U. Kunze, and A. D. Wieck, “Layer-compensated selectively doped AlxG-xAs/GaAs heterostructures as a base material for nanolithography,” Semiconductor Science and Technology, pp. 603–607, 2002.

G. Meschut, “Hybridfügen – Grundlagen, Technologie, Anwendungen,” in DVM-Bericht 668, Berlin, 2001, vol. 668, pp. 119–134.

J. Fromme, S. Ganguin, S. Iske, D. M. Meister, and U. Sander, Eds., Medienbildung und Gesellschaft. VS Verlag, 2000.

M. Koyro and G. Meschut, “Eine quasistationäre Meßmethode zur Ermittlung der Wärmeleitfähigkeit polymerer Zwischenschichten in Abhängigkeit von der Temperatur,” in Tagungsband zur Veranstaltung Werkstoffprüfung 1999, 1999, pp. 173–184.

T. Meier et al., “Coherent Dynamics of Exciton Wavepackets in Semiconductor Heterostructures,”10.1088/0268-1242/9/11S/018__in Proceedings der 8. International Winterschool on New Developments in Physics, Mauterndorf, 1994, vol. 9, no. 11S, pp. 1965–1971, doi:10.1088/0268-1242/9/11S/018 .