Evaluation of anti-adhesive and corrosion protection properties of TiAlSiN-magnetron-sputtered films for applications in polymer processing
C. Theile-Rasche, F. Wang, T. Prüßner, M. Huck, H.-G. Steinrück, M.T. de los Arcos de Pedro, G. Grundmeier, Thin Solid Films 820 (2025).

Optical properties of silicon oxynitride films grown by plasma-enhanced chemical vapor deposition
R. Aschwanden, R. Köthemann, M. Albert, C. Golla, C. Meier, Thin Solid Films 736 (2021).

Reducing the Schottky barrier height at the MoSe2/Mo(110) interface in thin-film solar cells: Insights from first-principles calculations
H. Mirhosseini, J. Kiss, G. Roma, C. Felser, Thin Solid Films (2016) 143–147.

Spectroelectrochemical and morphological studies of the ageing of silver nanoparticles embedded in ultra-thin perfluorinated sputter deposited films
C. Ebbert, N. Alissawi, C. Somsen, G. Eggeler, T. Strunskus, F. Faupel, G. Grundmeier, Thin Solid Films (2014) 161–167.

Lift-off of mesoporous layers by electrochemical etching on Si (100) substrates with miscut of 6° off towards (111)
E. Garralaga Rojas, B. Terheiden, H. Plagwitz, J. Hensen, V. Wiedemeier, G. Berth, A. Zrenner, R. Brendel, Thin Solid Films 520 (2011) 606–609.

Influence of process parameters on the crystallinity, morphology and composition of tungsten oxide-based thin films grown by metalorganic chemical vapor deposition
M.T. de los Arcos de Pedro, S. Cwik, A.P. Milanov, V. Gwildies, H. Parala, T. Wagner, A. Birkner, D. Rogalla, H.-W. Becker, J. Winter, A. Ludwig, R.A. Fischer, A. Devi, Thin Solid Films (2011) 11–16.

X-ray photoelectron spectroscopy on implanted argon as a tool to follow local structural changes in thin films
A.R. Lahrood, M.T. de los Arcos de Pedro, M. Prenzel, A. von Keudell, J. Winter, Thin Solid Films (2011) 1625–1630.

X-ray absorption near-edge spectroscopy investigation of the oxidation state of Pd species in nanoporous SnO2 gas sensors for methane detection
T. Wagner, M. Bauer, T. Sauerwald, C.-D. Kohl, M. Tiemann, Thin Solid Films (2011) 909–912.

Photocatalytic ozone sensor based on mesoporous indium oxide: Influence of the relative humidity on the sensing performance
T. Wagner, J. Hennemann, C.-D. Kohl, M. Tiemann, Thin Solid Films (2011) 918–921.

Gas sensor based on ordered mesoporous In2O3
T. Wagner, T. Sauerwald, C.-D. Kohl, T. Waitz, C. Weidmann, M. Tiemann, Thin Solid Films (2009) 6170–6175.

Ordered mesoporous ZnO for gas sensing
T. Wagner, T. Waitz, J. Roggenbuck, M. Fröba, C.-D. Kohl, M. Tiemann, Thin Solid Films (2007) 8360–8363.

Calculation of surface optical properties: from qualitative understanding to quantitative predictions
W.G. Schmidt, K. Seino, P.H. Hahn, F. Bechstedt, W. Lu, S. Wang, J. Bernholc, Thin Solid Films 455–456 (2004) 764–771.

Diamond (111) and (100) surface reconstructions
A. Scholze, W.G. Schmidt, F. Bechstedt, Thin Solid Films 281–282 (1996) 256–259.