Conversion between detector- and rotary-table-related misalignment parameterisations for unified projection-matrix-based geometry calibration in dimensional X-ray computed tomography
L. Butzhammer, Precision Engineering 100 (2026) 377–400.