A composite consisting of intermetallic Ni3Fe and nitrogen-doped carbon for electrocatalytic water oxidation: The effect of increased pyridinic nitrogen dopant
D. Liu, H. Zhai, J. Hu, Y. Pan, G. Xu, C. Zhu, Y. Yuan, Ceramics International 48 (2021) 5759–5765.