Power-to-hydrogen and hydrogen-to-X energy systems for the industry of the future in Europe
M. Genovese, A. Schlüter, E. Scionti, F. Piraino, O. Corigliano, P. Fragiacomo, International Journal of Hydrogen Energy 48 (2023) 16545–16568.
LibreCat: /record/52204
DOI: 10.1016/j.ijhydene.2023.01.194

Model-based design of a segmented reactor for the flexible operation of the methanation of CO2
F. Herrmann, M. Grünewald, J. Riese, International Journal of Hydrogen Energy 48 (2022) 9377–9389.
LibreCat: /record/47552
DOI: 10.1016/j.ijhydene.2022.12.122

Kinetic studies of cathode degradation as caused by ice formation in MEAs
L. Liphardt, S. Disson, K. Suematsu, G. Grundmeier, International Journal of Hydrogen Energy (2020) 23151–23159.
LibreCat: /record/22828
DOI: 10.1016/j.ijhydene.2020.05.270

Kinetic studies of cathode degradation on PEM fuel cell short stack level undergoing freeze startups with different states of residual water and current draws
L. Liphardt, K. Suematsu, G. Grundmeier, International Journal of Hydrogen Energy 46 (2020) 4399–4406.
LibreCat: /record/34643
DOI: 10.1016/j.ijhydene.2020.10.273

BrOx cycle: A novel process for CO2-free energy production from natural gas
J. González Rebordinos, A.H.J. Salten, D.W. Agar, International Journal of Hydrogen Energy 42 (2017) 4710–4720.
LibreCat: /record/22288
DOI: 10.1016/j.ijhydene.2016.09.071