Light-activated resistive ozone sensing at room temperature utilizing nanoporous In2O3 particles: Influence of particle size
D. Klaus, D. Klawinski, S. Amrehn, M. Tiemann, T. Wagner, Sensors and Actuators B: Chemical (2015) 181–185.
LibreCat: /record/25941
DOI: 10.1016/j.snb.2014.09.021

Nanostructured Co3O4 as a CO gas sensor: Temperature-dependent behavior
S. Vetter, S. Haffer, T. Wagner, M. Tiemann, Sensors and Actuators B: Chemical (2015) 133–138.
LibreCat: /record/25942
DOI: 10.1016/j.snb.2014.09.025

UV light-enhanced NO2 sensing by mesoporous In2O3: Interpretation of results by a new sensing model
T. Wagner, C.-D. Kohl, C. Malagù, N. Donato, M. Latino, G. Neri, M. Tiemann, Sensors and Actuators B: Chemical (2013) 488–494.
LibreCat: /record/25954
DOI: 10.1016/j.snb.2013.02.025

Micrometer-sized nanoporous tin dioxide spheres for gas sensing
J.-H. Smått, M. Lindén, T. Wagner, C.-D. Kohl, M. Tiemann, Sensors and Actuators B: Chemical (2011) 483–488.
LibreCat: /record/25963
DOI: 10.1016/j.snb.2010.12.051

Ordered nanoporous SnO2 gas sensors with high thermal stability
T. Waitz, B. Becker, T. Wagner, T. Sauerwald, C.-D. Kohl, M. Tiemann, Sensors and Actuators B: Chemical (2010) 788–793.
LibreCat: /record/25967
DOI: 10.1016/j.snb.2010.08.001