Klaus, D., Klawinski, D., Amrehn, S., Tiemann, M., &; Wagner, T. (2015). Light-activated resistive ozone sensing at room temperature utilizing nanoporous In2O3 particles: Influence of particle size. Sensors and Actuators B: Chemical, 181–185.https://doi.org/10.1016/j.snb.2014.09.021 

Vetter, S., Haffer, S., Wagner, T., &; Tiemann, M. (2015). Nanostructured Co3O4 as a CO gas sensor: Temperature-dependent behavior. Sensors and Actuators B: Chemical, 133–138.https://doi.org/10.1016/j.snb.2014.09.025 

Wagner, T., Kohl, C.-D., Malagù, C., Donato, N., Latino, M., Neri, G., &; Tiemann, M. (2013). UV light-enhanced NO2 sensing by mesoporous In2O3: Interpretation of results by a new sensing model. Sensors and Actuators B: Chemical, 488–494.https://doi.org/10.1016/j.snb.2013.02.025 

Smått, J.-H., Lindén, M., Wagner, T., Kohl, C.-D., &; Tiemann, M. (2011). Micrometer-sized nanoporous tin dioxide spheres for gas sensing. Sensors and Actuators B: Chemical, 483–488.https://doi.org/10.1016/j.snb.2010.12.051 

Waitz, T., Becker, B., Wagner, T., Sauerwald, T., Kohl, C.-D., &; Tiemann, M. (2010). Ordered nanoporous SnO2 gas sensors with high thermal stability. Sensors and Actuators B: Chemical, 788–793.https://doi.org/10.1016/j.snb.2010.08.001