2.38 Tbit/s, 1.49 bit/s/Hz, and (160 Gbit/s) RZ-DQPSK polarization division multiplex transmission over 273 km of fiber
A. Abas, B. Milivojevic, A. Hidayat, S. Bhandare, D. Sandel, H. Zhang, R. Noé, ELECTRICAL ENGINEERING 88 (2006) 211–214.

Design of a tunable optical chromatic dispersion compensator with simplified control of a Mach-Zehnder lattice, and dispersion slope mitigation
R. Noé, Z. Gao, ELECTRICAL ENGINEERING 86 (2004) 165–169.

Design of a tunable optical chromatic dispersion compensator with simplified control of a Mach-Zehnder lattice, and dispersion slope mitigation
R. Noé, Z. Gao, ELECTRICAL ENGINEERING 86 (2004) 165–169.

Robust, signed, online chromatic dispersion detection in a 40-Gbit/s optical transmission link
D. Sandel, V. Mirvocla, F. Wust, R. Noé, ELECTRICAL ENGINEERING 85 (2003) 41–44.

Linear detection of optical polarization mode dispersion by arrival time modulation
V. Mirvoda, D. Sandel, F. Wust, S. Hinz, R. Noé, ELECTRICAL ENGINEERING 84 (2002) 71–73.

Linear detection of optical polarization mode dispersion by arrival time modulation
V. Mirvoda, D. Sandel, F. Wust, S. Hinz, R. Noé, ELECTRICAL ENGINEERING 84 (2002) 71–73.

Optical amplifier performance in digital optical communication systems
R. Noé, ELECTRICAL ENGINEERING 83 (2001) 15–20.

Tolerance of bandwidth-efficient optical multilevel modulation schemes against polarization mode dispersion
S. Hinz, R. Noé, D. Sandel, F. Wust, ELECTRICAL ENGINEERING 83 (2001) 129–132.

Optical amplifier performance in digital optical communication systems
R. Noé, ELECTRICAL ENGINEERING 83 (2001) 15–20.

Tolerance of bandwidth-efficient optical multilevel modulation schemes against polarization mode dispersion
S. Hinz, R. Noé, D. Sandel, F. Wust, ELECTRICAL ENGINEERING 83 (2001) 129–132.