Bhandare, S., et al. “.6-Tb/s (40 Gb/s) Transmission over 44, ..., 94 Km of SSMF with Adaptive Chromatic Dispersion Compensation.”10.1109/LPT.2005.859522__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 17, no. 12, 2005, pp. 2748–50, doi:10.1109/LPT.2005.859522.

Milivojevic, B., et al. “.6-b/s/Hz 160-Gb/s 230-Km RZ-DQPSK Polarization Multiplex Transmission with Tunable Dispersion Compensation.”10.1109/LPT.2004.839372__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 17, no. 2, 2005, pp. 495–97, doi:10.1109/LPT.2004.839372.

Bhandare, S., et al. “.94-Tb/s 1.49-b/s/Hz (40 x 2 x 2 x 40 Gb/s) RZ-DQPSK Polarization-Division Multiplex C-Band Transmission over 324 Km.”10.1109/LPT.2005.843962__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 17, no. 4, 2005, pp. 914–16, doi:10.1109/LPT.2005.843962.

Noé, Reinhold. “PLL-Free Synchronous QPSK Polarization Multiplex/Diversity Receiver Concept with Digital I&;Q Baseband Processing.”10.1109/LPT.2004.842795__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 17, no. 4, 2005, pp. 887–89, doi:10.1109/LPT.2004.842795.

Noé, Reinhold. “PLL-Free Synchronous QPSK Polarization Multiplex/Diversity Receiver Concept with Digital I&;Q Baseband Processing.”10.1109/LPT.2004.842795__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 17, no. 4, 2005, pp. 887–89, doi:10.1109/LPT.2004.842795.

Sandel, D., et al. “Automatic Tunable Chromatic Dispersion Compensation at 40 Gb/s in ASK and DPSK, NRZ, and CSRZ 263-Km Transmission Experiments.”10.1109/LPT.2004.834889__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 16, no. 11, 2004, pp. 2568–70, doi:10.1109/LPT.2004.834889.

Noé, Reinhold, and D. Sandel. “Strategies for Fast Control Speed and DC Drift Avoidance in Distributed LiNbO3-Based PMD Compensators.”10.1109/LPT.2004.824959__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 16, no. 4, 2004, pp. 1050–52, doi:10.1109/LPT.2004.824959.

Noé, Reinhold, and D. Sandel. “Strategies for Fast Control Speed and DC Drift Avoidance in Distributed LiNbO3-Based PMD Compensators.”10.1109/LPT.2004.824959__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 16, no. 4, 2004, pp. 1050–52, doi:10.1109/LPT.2004.824959.

Sandel, D., et al. “Standard (NRZ 1 x 40 Gb/s, 210 Km) and Polarization Multiplex (CS-RZ, 2 x 40 Gb/s, 212 Km) Transmissions with PMD Compensation.”10.1109/LPT.2002.1022011__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 14, no. 8, 2002, pp. 1181–83, doi:10.1109/LPT.2002.1022011.

Sandel, D., et al. “Standard (NRZ 1 x 40 Gb/s, 210 Km) and Polarization Multiplex (CS-RZ, 2 x 40 Gb/s, 212 Km) Transmissions with PMD Compensation.”10.1109/LPT.2002.1022011__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 14, no. 8, 2002, pp. 1181–83, doi:10.1109/LPT.2002.1022011.

Noé, Reinhold, and K. DROGEMULLER. “ACCURATE AND SIMPLE OPTICAL FREQUENCY STABILIZATION FOR A COHERENT MULTICHANNEL SYSTEM.”10.1109/68.136502__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 4, no. 5, 1992, pp. 505–06, doi:10.1109/68.136502.

Noé, Reinhold, et al. “DIRECT MODULATION 565 MB/S DPSK EXPERIMENT WITH 62.3 DB LOSS SPAN AND ENDLESS POLARIZATION CONTROL.”10.1109/68.163762__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 4, no. 10, 1992, pp. 1151–54, doi:10.1109/68.163762.

Noé, Reinhold, et al. “OPTICAL AMPLIFIER WITH 27-DB DYNAMIC-RANGE IN A COHERENT TRANSMISSION-SYSTEM.”10.1109/68.47067__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 2, no. 2, 1990, pp. 120–21, doi:10.1109/68.47067.

Noé, Reinhold, et al. “OPTICAL AMPLIFIER WITH 27-DB DYNAMIC-RANGE IN A COHERENT TRANSMISSION-SYSTEM.”10.1109/68.47067__IEEE PHOTONICS TECHNOLOGY LETTERS, vol. 2, no. 2, 1990, pp. 120–21, doi:10.1109/68.47067.