Process window expansion with transferable applicability in three-layer dissimilar steel resistance spot welding via expulsion prevention
K. Yang, L. Männer, Z. Wang, V. Olfert, Y. Böhm, D. Hein, G. Meschut, Journal of Manufacturing Processes 157 (2026) 984–1000.

Predictive modeling of tolerance-dependent failure behavior of self-pierce riveted joints: From coupon-level tests to sub-component validation
V. Olfert, K. Yang, P. Rochel, P. Bähr, D. Hein, S. Sommer, G. Meschut, Journal of Manufacturing Processes 157 (2026) 1250–1273.

A physics-guided hybrid framework for online pre-expulsion prediction in resistance spot welding
K. Yang, C. Li, R. Beck, D. Hein, G. Meschut, Journal of Manufacturing Processes 174 (2026) 135–153.

Single-step self-punching lockbolt process and equipment development for pre-hole-free joining of aluminum sheets using a dual-die system
Y. Böhm, F. Kappe, D. Han, E. Nordmann, K. Yang, J. Jendrny, E. Gorr, G. Meschut, Journal of Manufacturing Processes 155 (2025) 171–184.

From simulation to metamodel to experiment: Evaluating the prediction accuracy of polynomial regression models for clinch joint properties
J.-M. Einwag, C. Steinfelder, S. Wartzack, A. Brosius, S. Goetz, Journal of Manufacturing Processes 154 (2025) 179–191.

A novel welding schedule for expanding the expulsion-free process window in resistance spot welding of dissimilar joints with ultra-high strength steel
K. Yang, Z. Wang, V. Haak, V. Olfert, B. El-Sari, D. Hein, M. Biegler, M. Rethmeier, G. Meschut, Journal of Manufacturing Processes 137 (2025) 306–319.

Single-step self-punching lockbolt process for aluminum sheets without pre-hole
D. Han, F. Kappe, J. Vorderbrüggen, J. Jendrny, E. Gorr, G. Meschut, Journal of Manufacturing Processes 116 (2024) 92–108.

Expulsion prevention in resistance spot welding of dissimilar joints with ultra-high strength steel: An analysis of the mechanism and effect of preheating current
K. Yang, B. El-Sari, V. Olfert, Z. Wang, M. Biegler, M. Rethmeier, G. Meschut, Journal of Manufacturing Processes 124 (2024) 489–502.

Determining the influence of different process parameters on the versatile self-piercing riveting process using numerical methods
F. Kappe, C. Zirngibl, B. Schleich, M. Bobbert, S. Wartzack, G. Meschut, Journal of Manufacturing Processes 84 (2022) 1438–1448.

Deformation of expanded steel mesh inlay inside aluminum matrix during the roll bonding
Y. Frolov, Y. Haranich, O. Bobukh, O. Remez, D. Voswinkel, O. Grydin, Journal of Manufacturing Processes 58 (2020) 857–867.