A novel welding schedule for expanding the expulsion-free process window in resistance spot welding of dissimilar joints with ultra-high strength steel
K. Yang, Z. Wang, V. Haak, V. Olfert, B. El-Sari, D. Hein, M. Biegler, M. Rethmeier, G. Meschut, Journal of Manufacturing Processes 137 (2025) 306–319.

Single-step self-punching lockbolt process for aluminum sheets without pre-hole
D. Han, F. Kappe, J. Vorderbrüggen, J. Jendrny, E. Gorr, G. Meschut, Journal of Manufacturing Processes 116 (2024) 92–108.

Expulsion prevention in resistance spot welding of dissimilar joints with ultra-high strength steel: An analysis of the mechanism and effect of preheating current
K. Yang, B. El-Sari, V. Olfert, Z. Wang, M. Biegler, M. Rethmeier, G. Meschut, Journal of Manufacturing Processes 124 (2024) 489–502.

Determining the influence of different process parameters on the versatile self-piercing riveting process using numerical methods
F. Kappe, C. Zirngibl, B. Schleich, M. Bobbert, S. Wartzack, G. Meschut, Journal of Manufacturing Processes 84 (2022) 1438–1448.

Deformation of expanded steel mesh inlay inside aluminum matrix during the roll bonding
Y. Frolov, Y. Haranich, O. Bobukh, O. Remez, D. Voswinkel, O. Grydin, Journal of Manufacturing Processes 58 (2020) 857–867.