Fracture mechanical evaluation of the material HX
B. Schramm, D. Weiß, Materials Testing 64 (2022) 1437–1449.

Influence of various procedures for the determination of flow curves on the predictive accuracy of numerical simulations for mechanical joining processes
M. Böhnke, F. Kappe, M. Bobbert, G. Meschut, Materials Testing 63 (2021) 493–500.

Increased load bearing capacity of mechanically joined FRP/metal joints using a pin structured auxiliary joining element
P. Heyser, V. Sartisson, G. Meschut, M. Droß, K. Dröder, Materials Testing (2020) 55–60.

Early stage crack detection in mechanically joined steel/aluminum joints by condition monitoring
M. Gollnick, P. Giese, D. Hein, G. Meschut, D. Herfert, Materials Testing 62 (2020) 877–882.

Testing of pipe sections
A. Andreiev, O. Golovko, I. Frolov, F. Nürnberger, L.O. Wolf, M. Schaper, O. Grydin, Materials Testing (2015) 643–648.

Verhalten von lasergeschmolzenen Bauteilen aus der Titan-Aluminium-Legierung TiAl6 unter zyklischer Beanspruchung
A. Riemer, S. Leuders, H.A. Richard, T. Tröster, Materials Testing (2013) 537–543.

Einsatz von Simulationswerkzeugen in der Entwicklungskette von ultrahochfesten warmgeformten Strukturkomponenten im Fahrzeugleichtbau*
J. Böke, R. Erhardt, W. Rostek, T. Tröster, Materials Testing (2009) 22–27.