Fracture mechanical investigation of preformed metal sheets using a novel CC-specimen
D. Weiß, B. Schramm, in: Procedia Structural Integrity, Elsevier BV, 2022, pp. 879–885.

Influence of plane mixed-mode loading on the kinking angle of clinchable metal sheets
D. Weiß, B. Schramm, G. Kullmer, in: Procedia Structural Integrity, Elsevier BV, 2022, pp. 139–147.

Fatigue strength of adhesively butt-bonded hollow cylinders under multiaxial loading with constant and variable amplitudes
M. Hecht, J. Baumgartner, K. Tews, S. Çavdar, G. Meschut, Procedia Structural Integrity 38 (2022) 251–259.

Fracture prediction of additively manufactured AlSi10Mg materials
E.F. Akbulut Irmak, T. Tröster, Procedia Structural Integrity (2019) 190–197.

Fatigue crack growth behavior and mechanical properties of additively processed EN AW-7075 aluminium alloy
W. Reschetnik, J.-P. Brüggemann, M.E. Aydinöz, O. Grydin, K.-P. Hoyer, G. Kullmer, H.A. Richard, Procedia Structural Integrity (2016) 3040–3048.

Fatigue crack growth behavior and mechanical properties of additively processed EN AW-7075 aluminium alloy
W. Reschetnik, J.-P. Brüggemann, M.E. Aydinöz, O. Grydin, K.-P. Hoyer, G. Kullmer, H.-A. Richard, Procedia Structural Integrity 2 (2016) 3040–3048.