Fe and Sn Single-Site-Based Electrodes for High-Current CO<sub>2</sub> Reduction in Acid Media and Stable Zn–CO<sub>2</sub> Batteries
J. Hu, S. Goberna-Ferrón, L. Simonelli, N. Lopez-Salas, H. García, J. Albero, ACS Applied Energy Materials 8 (2025) 1179–1188.

Combined Effects of Uniform Applied Pressure and Electrolyte Additives in Lithium-Metal Batteries
R.M. Kasse, N.R. Geise, E. Sebti, K. Lim, C.J. Takacs, C. Cao, H.-G. Steinrück, M.F. Toney, ACS Applied Energy Materials 5 (2022) 8273–8281.

Using In Situ High-Energy X-ray Diffraction to Quantify Electrode Behavior of Li-Ion Batteries from Extreme Fast Charging
P.P. Paul, C. Cao, V. Thampy, H.-G. Steinrück, T.R. Tanim, A.R. Dunlop, S.E. Trask, A.N. Jansen, E.J. Dufek, J. Nelson Weker, M.F. Toney, ACS Applied Energy Materials 4 (2021) 11590–11598.