Influence of the Deposition Rate on the Alignment and Performance of Perylene-3,4,9,10-tetracarboxylic Tetraethyl Ester in an Organic Light Emitting Diode
D. Becker, P. Meier, A. Kuhlmann, C. Sternemann, H. Bock, H.-G. Steinrück, H.-S. Kitzerow, ACS Applied Electronic Materials 6 (2024) 1234–1243.