Controlling the helicity of light by electrical magnetization switching
P.A. Dainone, N.F. Prestes, P. Renucci, A. Bouché, M. Morassi, X. Devaux, M. Lindemann, J.-M. George, H. Jaffrès, A. Lemaitre, B. Xu, M. Stoffel, T. Chen, L. Lombez, D. Lagarde, G. Cong, T. Ma, P. Pigeat, M. Vergnat, H. Rinnert, X. Marie, X. Han, S. Mangin, J.-C. Rojas-Sánchez, J.-P. Wang, M.C. Beard, N.C. Gerhardt, I. duti, Y. Lu, Nature 627 (2024) 783–788.

SpinLasing in Bimodal Quantum Dot Micropillar Cavities
N. Heermeier, T. Heuser, J. Große, N. Jung, A. Kaganskiy, M. Lindemann, N.C. Gerhardt, M.R. Hofmann, S. Reitzenstein, Laser &;amp; Photonics Reviews 16 (2022).

Analysis of the effects of jitter, relative intensity noise, and nonlinearity on a photonic digital-to-analog converter based on optical Nyquist pulse synthesis
C. Kress, M. Bahmanian, T. Schwabe, J.C. Scheytt, Opt. Express 29 (2021) 23671–23681.

Tunable femtosecond near-IR source by pumping an OPA directly with a 90 MHz Yb:fiber source
J. Mundry, J. Lohrenz, M. Betz, Applied Optics 56 (2017) 3104–3108.