A Newton-Multigrid algrithm for elasto-plastic/viscoplastic problems
R. Mahnken, Computational Mechanics 15 (2008) 408–425.

Dichroic photo- and electroluminescence of oligo p-(phenylene vinylene) derivatives
M.W. Lauhof, S.A. Benning, H.-S. Kitzerow, V. Vill, F. Scheliga, E. Thorn-Csányi, Synthetic Metals 157 (2007) 222–227.

Spin-electronic devices with half-metallic Heusler alloys
A. Hütten, J. Schmalhorst, A. Thomas, S. Kämmerer, M. Sacher, D. Ebke, N.-N. Liu, X. Kou, G. Reiss, Journal of Alloys and Compounds 423 (2006) 148–152.

Degradation of organic field-effect transistors made of pentacene
Ch. Pannemann, T. Diekmann, U. Hilleringmann, Journal of Materials Research 19 (2005) 1999–2002.

Degradation of organic field-effect transistors made of pentacene
Ch. Pannemann, T. Diekmann, U. Hilleringmann, Journal of Materials Research 19 (2005) 1999–2002.

Director reorientation of a side-chain liquid crystalline polymer under extensional flow
R.J. Cormier, C. Schmidt, P.T. Callaghan, Journal of Rheology 48 (2004) 881–894.

Morphology and fluorescence quenching in photovoltaic samples containing fullerene and poly(p-phenylene-vinylene) derivatives
T. Röder, H.-S. Kitzerow, J.C. Hummelen, Synthetic Metals 141 (2003) 271–275.

Structures with a minimum feature size of less than 100 nm in CVD-diamond for sensor applications
R. Otterbach, U. Hilleringmann, T.J. Horstmann, K. Goser, Diamond and Related Materials 10 (2002) 511–514.

Reactive ion etching of CVD-diamond for piezoresistive pressure sensors
R. Otterbach, U. Hilleringmann, Diamond and Related Materials 11 (2002) 841–844.

Strength difference in compression and tension and pressure dependence of yielding in elasto-plasticity
R. Mahnken, Computer Methods in Applied Mechanics and Engineering 190 (2002) 5057–5080.