Adaptive DC-Link Voltage Control for 22 kW, 40 kHz LLC Resonant Converter Considering Low-Frequency Voltage Ripple
R. Unruh, J. Böcker, F. Schafmeister, Electronics 14 (2025).

An Optimized Third-Harmonic Injection Reduces DC-Link Voltage Ripple in Cascaded H-Bridge Converters up to 50% for all Power Factors
R. Unruh, J. Böcker, F. Schafmeister, in: 2023 25th European Conference on Power Electronics and Applications (EPE’23 ECCE Europe), IEEE, 2023.

Template-induced graphitic nanodomains in nitrogen-doped carbons enable high-performance sodium-ion capacitors - ACCEPTED MANUSCRIPT
N. Lopez Salas, C. Li, Z. Song, M. Liu, E. Lepre, M. Antonietti, J. Zhu, J. Liu, Y. Fu, (2023).

Zero-Sequence Voltage Reduces DC-Link Capacitor Demand in Cascaded H-Bridge Converters for Large-Scale Electrolyzers by 40%
R. Unruh, F. Schafmeister, J. Böcker, in: 24th European Conference on Power Electronics and Applications (EPE’22 ECCE Europe), IEEE, 2022.

1-MW Full-Bridge MMC for High-Current Low-Voltage (100V-400V) DC-Applications
R. Unruh, F. Schafmeister, N. Fröhleke, J. Böcker, in: PCIM Europe Digital Days 2020; International Exhibition and Conference for Power Electronics, Intelligent Motion, Renewable Energy and Energy Management, VDE, 2020.

A simple pre-stress estimating method of langevin transducers
F. Bo, L. Ting, T. Hemsel, in: Piezoelectricity, Acoustic Waves, and Device Applications, 2008. SPAWDA 2008. Symposium On, 2008, pp. 324–327.