Self-Piercing Riveting Using Rivets Made of Stainless Steel with High Strain Hardening
B. Uhe, C.-M. Kuball, M. Merklein, G. Meschut, in: G. Daehn, J. Cao, B. Kinsey, E. Tekkaya, A. Vivek, Y. Yoshida (Eds.), Forming the Future - Proceedings of the 13th International Conference on the Technology of Plasticity. The Minerals, Metals &; Materials Series., Springer, Cham, 2021, pp. 1495–1506.

Investigation of wear resistance of dry and cryogenic turned metastable austenitic steel shafts and dry turned and ground carburized steel shafts in the radial shaft seal ring system
D. Frölich, B. Magyar, B. Sauer, P. Mayer, B. Kirsch, J.C. Aurich, R. Skorupski, M. Smaga, T. Beck, D. Eifler, Wear 328–329 (2015) 123–131.

Improving the bond quality of copper wire bonds using a friction model approach
S. Althoff, J. Neuhaus, T. Hemsel, W. Sextro, in: Electronic Components and Technology Conference (ECTC), 2014 IEEE 64th, 2014, pp. 1549–1555.

Experimental and Numerical Simulation Study of Pre-Deformed Heavy Copper Wire Wedge Bonds
A. Unger, W. Sextro, S. Althoff, P. Eichwald, T. Meyer, F. Eacock, M. Brökelmann, in: Proceedings of the 47th International Symposium on Microelectronics (IMAPS), San Diego, CA, US, 2014, pp. 289–294.