Expulsion prevention in resistance spot welding of dissimilar joints with ultra-high strength steel: An analysis of the mechanism and effect of preheating current
K. Yang, B. El-Sari, V. Olfert, Z. Wang, M. Biegler, M. Rethmeier, G. Meschut, Journal of Manufacturing Processes 124 (2024) 489–502.

3D-structure of intermetallic interface layer in Al–steel clad material
M. Slapáková, B. Kihoulou, J. Veselý, P. Minárik, K. Fekete, M. Knapek, R. Králík, O. Grydin, M. Stolbchenko, M. Schaper, Vacuum 212 (2023).

Integrating Prospective LCA in the Development of Automotive Components
J. Grenz, M. Ostermann, K. Käsewieter, F. Cerdas, T. Marten, C. Herrmann, T. Tröster, Sustainability 15 (2023).

Experimental failure analysis of adhesively bonded steel/CFRP joints under quasi-static and cyclic tensile-shear and peel loading
J. Kowatz, D. Teutenberg, G. Meschut, International Journal of Adhesion and Adhesives 107 (2021).

Forming of metastable austenitic stainless steel tubes with axially graded martensite content by flow-forming
B. Arian, W. Homberg, M. Riepold, A. Trächtler, J. Rozo Vasquez, F. Walther, in: ULiège Library, Liège, 2021.

Investigation of wear resistance of dry and cryogenic turned metastable austenitic steel shafts and dry turned and ground carburized steel shafts in the radial shaft seal ring system
D. Frölich, B. Magyar, B. Sauer, P. Mayer, B. Kirsch, J.C. Aurich, R. Skorupski, M. Smaga, T. Beck, D. Eifler, Wear 328–329 (2015) 123–131.