Dichroic photo- and electroluminescence of oligo p-(phenylene vinylene) derivatives
M.W. Lauhof, S.A. Benning, H.-S. Kitzerow, V. Vill, F. Scheliga, E. Thorn-Csányi, Synthetic Metals 157 (2007) 222–227.

Piezoelectric linear motor concepts based on coupling of longitudinal vibrations
T. Hemsel, M. Mracek, J. Twiefel, P. Vasiljev, Ultrasonics 44, Supplement (2006) e591–e596.

Synergetic driving concepts for bundled miniature ultrasonic linear motors
M. Mracek, T. Hemsel, Ultrasonics 44, Supplement (2006) e597–e602.

Perceptual latency priming and illusory line motion: Facilitation by gradients of attention?
I. Scharlau, G. Horstmann, Advances in Cognitive Psychology 2 (2006) 87–97.

Spin-electronic devices with half-metallic Heusler alloys
A. Hütten, J. Schmalhorst, A. Thomas, S. Kämmerer, M. Sacher, D. Ebke, N.-N. Liu, X. Kou, G. Reiss, Journal of Alloys and Compounds 423 (2006) 148–152.

System-level performance evaluation of reconfigurable processors
R. Enzler, C. Plessl, M. Platzner, Microprocessors and Microsystems 29 (2005) 63–73.

A Model-Based Approach for Executable Specification on Reconfigurable Hardware
T. Schattkowsky, W. Müller, A. Rettberg, in: Proceedings of DATE’05, IEEE, Munich, Germany , 2005.

Degradation of organic field-effect transistors made of pentacene
Ch. Pannemann, T. Diekmann, U. Hilleringmann, Journal of Materials Research 19 (2005) 1999–2002.

Degradation of organic field-effect transistors made of pentacene
Ch. Pannemann, T. Diekmann, U. Hilleringmann, Journal of Materials Research 19 (2005) 1999–2002.

A novel approach for high power ultrasonic linear motors
T. Hemsel, M. Mracek, J. Wallaschek, P. Vasiljev, in: Ultrasonics Symposium, 2004 IEEE, 2004, pp. 1161–1164.

Director reorientation of a side-chain liquid crystalline polymer under extensional flow
R.J. Cormier, C. Schmidt, P.T. Callaghan, Journal of Rheology 48 (2004) 881–894.

Co-simulation of a Hybrid Multi-Context Architecture
R. Enzler, C. Plessl, M. Platzner, in: Proc. Int. Conf. on Engineering of Reconfigurable Systems and Algorithms (ERSA), CSREA Press, 2003, pp. 174–180.

Morphology and fluorescence quenching in photovoltaic samples containing fullerene and poly(p-phenylene-vinylene) derivatives
T. Röder, H.-S. Kitzerow, J.C. Hummelen, Synthetic Metals 141 (2003) 271–275.

Piezoelectric transformers - state of the art and development trends
T. Hemsel, W. Littmann, J. Wallaschek, in: Ultrasonics Symposium, 2002. Proceedings. 2002 IEEE, 2002, pp. 645–648.

Structures with a minimum feature size of less than 100 nm in CVD-diamond for sensor applications
R. Otterbach, U. Hilleringmann, T.J. Horstmann, K. Goser, Diamond and Related Materials 10 (2002) 511–514.

Reactive ion etching of CVD-diamond for piezoresistive pressure sensors
R. Otterbach, U. Hilleringmann, Diamond and Related Materials 11 (2002) 841–844.

Strength difference in compression and tension and pressure dependence of yielding in elasto-plasticity
R. Mahnken, Computer Methods in Applied Mechanics and Engineering 190 (2002) 5057–5080.

Finite element simulation for rock salt with dilatancy boundary coupled to fluid permeation
R. Mahnken, M. Kohlmeier, Computer Methods in Applied Mechanics and Engineering 190 (2002) 4259–4278.

Implicit integration scheme and its consistent linearization for an elastoplastic-damage model with application to concrete
R. Mahnken, D. Tikhomirov, E. Stein, Computers &;amp; Structures 75 (2002) 135–143.

Improved implementation of an algorithm for non-linear isotropic/kinematic hardening in elastoplasticity
R. Mahnken, Communications in Numerical Methods in Engineering 15 (2002) 745–754.