Process window expansion with transferable applicability in three-layer dissimilar steel resistance spot welding via expulsion prevention
K. Yang, L. Männer, Z. Wang, V. Olfert, Y. Böhm, D. Hein, G. Meschut, Journal of Manufacturing Processes 157 (2026) 984–1000.

Single-step self-punching lockbolt process and equipment development for pre-hole-free joining of aluminum sheets using a dual-die system
Y. Böhm, F. Kappe, D. Han, E. Nordmann, K. Yang, J. Jendrny, E. Gorr, G. Meschut, Journal of Manufacturing Processes 155 (2025) 171–184.