Jähn, Claudius, et al. “Evaluation of Rendering Algorithms Using Position-Dependent Scene Properties.”10.1007/978-3-642-41914-0_12__Advances in Visual Computing, 2013, doi:10.1007/978-3-642-41914-0_12.
LibreCat: /record/16406
DOI: 10.1007/978-3-642-41914-0_12

Petring, Ralf, et al. “Real-Time 3D Rendering of Heterogeneous Scenes.”10.1007/978-3-642-41914-0_44__Advances in Visual Computing, 2013, doi:10.1007/978-3-642-41914-0_44.
LibreCat: /record/16407
DOI: 10.1007/978-3-642-41914-0_44

Bause, F., et al. .2 - Design, Modeling and Identification of an Ultrasonic Composite Transducer for Target Impedance Independent Short Pulse Generation. LibreCat University, 2013, doi:10.5162/SENSOR2013/A3.2.
LibreCat: /record/13879
DOI: 10.5162/SENSOR2013/A3.2

Hoof, C., et al. 3.2 - Infrared Reflectance Measurements of Thin Films with Time Variable Surface Roughness or Texture. LibreCat University, 2013, doi:10.5162/OPTO2013/O3.2.
LibreCat: /record/13880
DOI: 10.5162/OPTO2013/O3.2

Rautenberg, Jens, et al. “Messsystem zur Bestimmung akustischer Kenngrößen stark absorbierender, transversal isotroper Kunststoffe.”10.1524/teme.2013.0005__tm - Technisches Messen, 2013, pp. 28–37, doi:10.1524/teme.2013.0005.
LibreCat: /record/13881
DOI: 10.1524/teme.2013.0005

Schmitt, Martin, et al. “Multi Reflection of Lamb Wave Emission in an Acoustic Waveguide Sensor.”10.3390/s130302777__Sensors, 2013, pp. 2777–85, doi:10.3390/s130302777.
LibreCat: /record/13882
DOI: 10.3390/s130302777

Schmitt, M., et al. “Detection of Coatings within Liquid-Filled Tubes and Containers by Mode Conversion of Leaky Lamb Waves.”10.5194/jsss-2-73-2013__Journal of Sensors and Sensor Systems, 2013, pp. 73–84, doi:10.5194/jsss-2-73-2013.
LibreCat: /record/13883
DOI: 10.5194/jsss-2-73-2013

Schröder, Andreas, and Bernd Henning. “Luftultraschall-Abstandsmessung mit digitaler Signalverarbeitung zur Verkürzung des Mindestabstandes.”10.1524/teme.2013.0022__tm - Technisches Messen, 2013, pp. 196–200, doi:10.1524/teme.2013.0022.
LibreCat: /record/13884
DOI: 10.1524/teme.2013.0022

Schröder, A., and Bernd Henning. .4 - Signal Processing for Single Transducer Distance Measurement Applications to Reduce the Blind Zone. LibreCat University, 2013, doi:10.5162/SENSOR2013/B5.4.
LibreCat: /record/13885
DOI: 10.5162/SENSOR2013/B5.4

Bause, Fabian, et al. Utilizing Ultrasound Material Parameter Determination for the Characterization of Different Stages of Ageing in Polyamide 6. 2013, pp. 504–09.
LibreCat: /record/13949