Wilfer, Claudia, et al. “Efficient Biomimetic Hydroxylation Catalysis with a Bis(Pyrazolyl)Imidazolylmethane Copper Peroxide Complex.”10.1002/chem.201501685__Chemistry - A European Journal, 2015, pp. 17639–49, doi:10.1002/chem.201501685.

Auroux, Sébastien, et al. “Dynamic Network Reconfiguration in Wireless DenseNets with the CROWD SDN Architecture.”10.1109/eucnc.2015.7194057__2015 European Conference on Networks and Communications (EuCNC), IEEE, 2015, doi:10.1109/eucnc.2015.7194057.

Klingler, Florian, et al. “MCB – A Multi-Channel Beaconing Protocol.”10.1016/j.adhoc.2015.08.002__Ad Hoc Networks, 2015, pp. 258–69, doi:10.1016/j.adhoc.2015.08.002.

Degener, Bastian, et al. “Linear and Competitive Strategies for Continuous Robot Formation Problems.”10.1145/2742341__ACM Transactions on Parallel Computing, 2015, pp. 1–18, doi:10.1145/2742341.

Abshoff, Sebastian, et al. “Towards Gathering Robots with Limited View in Linear Time: The Closed  Chain Case.” ArXiv: 1501.04877, 2015.

Olfert, Sergei, and Bernd Henning. Analyse Integral Erfasster Rotationssymmetrischer Schallwechseldruckverteilungen in Schlierenabbildungen. 15AD.

Kulshreshtha, Kshitij, et al. On the Optimal Configuration of Triple-Ring-Electrodes on Piezoceramic Transducers towards Increased Parameter Sensitivity of Impedance.

Olfert, Sergei, and Bernd Henning. “Analyse Integral Erfasster Schallwechseldruckverteilungen in Schlierenabbildungen.”10.1515/9783110408539-010__XXIX Messtechnisches Symposium, 2015, doi:10.1515/9783110408539-010.

Jurgelucks, Benjamin, et al. On the Optimal Configuration of Triple-Ring-Electrodes on Piezoceramic Transducers towards Increased Parameter Sensitivity of Impedance.

Bause, Fabian, et al. Model Based Sensitivity Analysis in the Determination of Viscoelastic Material Properties Using Transmission Measurements through Circular Waveguides. 2015, pp. 204–07.