Tebi, S., Aldahhak, H., Serrano, G., Schöfberger, W., Rauls, E., Schmidt, W. G.,https://doi.org/10.1088/0957-4484/27/2/025704__Müllegger, S. (2016). Manipulation resolves non-trivial structure of corrole monolayer on Ag(111). Nanotechnology, 27.https://doi.org/10.1088/0957-4484/27/2/025704 

Strotmeyer, S., John, T., &; Kundisch, D. (2016). Vergleichende Betrachtung von Software-Werkzeugen zur Geschäftsmodellentwicklung. In Multikonferenz Wirtschaftsinformatik (MKWI). Ilmenau, Germany.

Vollmers, D. (2016). Vergleich von Disambiguierungsansätzen bei Anforderungsbeschreibungen. Universität Paderborn.

Herlich, M., Bredenbals, N., &; Karl, H. (2016). Delayed (de-)activation in servers with a sleep mode. Sustainable Computing: Informatics and Systems, 10, 48–55.https://doi.org/10.1016/j.suscom.2016.04.002 

Paulheim, A., Marquardt, C., Sokolowski, M., Hochheim, M., Bredow, T., Aldahhak, H.,https://doi.org/10.1039/c6cp05661j__Schmidt, W. G. (2016). Surface induced vibrational modes in the fluorescence spectra of PTCDA adsorbed on the KCl(100) and NaCl(100) surfaces. Physical Chemistry Chemical Physics, 18, 32891–32902.https://doi.org/10.1039/c6cp05661j 

Yeom, H. W., Oh, D. M., Wippermann, S., &; Schmidt, W. G. (2016). Impurity-Mediated Early Condensation of a Charge Density Wave in an Atomic Wire Array. ACS Nano, 10, 810–814.https://doi.org/10.1021/acsnano.5b05925 

Adelt, P., Koppelmann, B., Müller, W., Becker, M., Kleinjohann, B., &; Scheytt, C. (2016). Fast Dynamic Fault Injection for Virtual Microcontroller Platforms. Proceedings of the IEEE/IFIP International Conference on VLSI (VLSI-SOC).https://doi.org/10.1109/VLSI-SoC.2016.7753545 

Mao, Y., Schmalz, K., Scheytt, C., &; Shiju, E. (2016). An all-transmission-line 220 GHz differential LNA in SiGe BiCMOS. IEEE International Symposium on Radio-Frequency Integration Technology.https://doi.org/10.1109/RFIT.2016.7578132 

Abughannam, S., Wu, L., Müller, W., Scheytt, C., Ecker, W., &; Novello, C. (2016). Fault Injection and Mixed-Level Simulation for Analog Circuits - A Case Study. Analog 2016 - VDE.

Nava, F., Genschow, D., &; Scheytt, C. (2016). Obstacle detection using a miniaturized radar sensor operating at 120GHz ISM band. DRONE Berlin 2016.