Plasma-Enhanced Chemical Vapor Deposition (PE-CVD) yields better Hydrolytical Stability of Biocompatible SiOx Thin Films on Implant Alumina Ceramics compared to Rapid Thermal Evaporation Physical Vapor Deposition (PVD)
F. Böke, I. Giner, A. Keller, G. Grundmeier, H. Fischer, ACS Applied Materials &; Interfaces 8 (2016) 17805–17816.