A Multi-Sensor Induction Flow Meter Reducing Errors due to Non-axisymmetric Flow Profiles
B. Horner, F. Mesch, A. Trächtler, Measurement Science and Technology 7 (1996) 354-360,.