Interferometric method for determining the losses of spatially multi-mode nonlinear waveguides based on second harmonic generation.
M. Santandrea, M. Stefszky, G. Roeland, C. Silberhorn, Optics Express 28 (2020).