Barkhausen Noise and Eddy CurrentBased Measurements for Online Detection of DeformationInduced Martensite During Flow Forming of Metastable Austenitic Steel <scp>AISI 304L</scp>
J. Rozo Vasquez, H. Kanagarajah, B. Arian, L. Kersting, W. Homberg, A. Trächtler, F. Walther, Engineering Reports 7 (2024).