Particle fouling at hot reactor walls monitored In situ with a QCM-D and modeled with the frequency-domain lattice Boltzmann method
D. Johannsmann, J. Petri, C. Leppin, A. Langhoff, H. Ibrahim, Results in Physics 45 (2023).