Increased electrical yield via water flow over the front of photovoltaic panels
S. Krauter, Solar Energy Materials &; Solar Cells 82 (2004) 1331–137.